|  |
| --- |
| **CE****EC Declaration of Performance** |
| Lime Green Products Ltd, Coates Kilns, Stretton Road, Much Wenlock, Shropshire, TF13 6DG15 |
| **Finish WP****EN 998–1:2010****Factory Made Coloured Rendering Mortar (CR) for external use****Reaction to fire:** Class B1**Strength Class**  CSII**Adhesion:** >0.08 (woodfibre)**Capillary Water absorption:** W2**Water vapour Permeability coefficient.** µ ≤10 **Thermal conductivity λ10,dry [W/mK] *P=50%*** 0.47 ***P= 90%*** 0.54**Durability (against freeze/thaw):** evaluation based on provisions valid in the intended place of use of the mortar |

**Date** 22/1/15

**Signed**

J Ayres – Director