|  |
| --- |
| **CE****EC Declaration of Performance** |
| Lime Green Products Ltd, Coates Kilns, Stretton Road, Much Wenlock, Shropshire, TF13 6DG13 |
| **EN 998–1:2010****Coloured Rendering mortar (CR) for external use****Reaction to fire:** Class A 1**Adhesion:** 0.7N/mm2 FP: b**Capillary Water absorption:** W1**Water vapour Permeability coefficient.** ≤15**Thermal conductivity λ10,dry [W/mK] *P=50%*** 0.83 ***P= 90%*** 0.93**Durability:** (against freeze/thaw)**:** evaluation based on provisions valid in the intended place of use of the mortar |

**Ionic Tradirend**

**Date** 9/7/2013

**Signed**

J Ayres – Director