|  |  |
| --- | --- |
| **EC Declaration of Performance** | **CE** |

The Producer

**Lime Green Products Ltd**

**Coates Kilns**

**Stretton Road**

**Much Wenlock**

**Shropshire**

**TF13 6DG**

Declares that the product

**Lime green Natural Lime Mortar - Strong**

Manufactured at

**Coates Kilns**

**Stretton Road**

**Much Wenlock**

**Shropshire**

**TF13 6DG**

Complies with the provisions of EN998-2 2010 and fulfils the conditions for CE marking in accordance with EN998-2 2010.

Evaluation of conformity has been carried out according to the procedures in table ZA.1

The product has undergone initial type testing and is subject to system 4 factory production control as specified in EN998-2.

**J Ayres**

**Director**

|  |
| --- |
| CE |
| Lime Green Products Ltd, Coates Kilns Stretton Road, Much Wenlock, Shropshire, TF13 6DG14 |
| EN 998-2 2010***Natural Lime Mortar - Strong***Prescribed general purpose mortar for internal and external use |
| **Proportion of constituents (by volume):**Hydraulic Lime (HL5) 1 Aggregates 2.5  |
| Reaction to fire | A1 |
| Water absorption kg/(m2.min0.5) | 1.19 |
| Water vapour permeability µ  | 15/35 |
| Thermal conductivity W/mK | P=50% 0.83 |
| Durability | Evaluation based on provisions valid in the intended place of use of the mortar |