|  |
| --- |
| **CE****EC Declaration of Performance** |
| Lime Green Products Ltd, Coates Kilns, Stretton Road, Much Wenlock, Shropshire, TF13 6DG13 |
| **Prepbond WP****EN 998–1:2010****Factory Made General Purpose Render for external use****Reaction to fire:** Class B1**Strength Class**  CSII**Adhesion:** >0.08 (woodfibre)**Capillary Water absorption:** W2**Water vapour Permeability coefficient.** µ **=** 5**Thermal conductivity λ10,dry [W/mK] *P=50%*** 0.30 ***P= 90%*** 0.36**Durability:** (against freeze/thaw)**:** evaluation based on provisions valid in the intended place of use of the mortar |

**Date** 3/12/14

**Signed**

J Ayres – Director