**EC Declaration of Performance**

1. Unique identification code of the product-type:

**Natural Finish**

2. Batch Number

**Printed batch code is on the side of packaging**

3. Intended use/es:

 **Coloured rendering mortar.**

4. Manufacturer:

**Lime Green Products Ltd**

**Coates Kilns**

**Stretton Road**

**Much Wenlock**

**Shropshire**

**TF13 6DG**

5. Authorised representative:

 **N/A**

6. System/s of AVCP:

 **System 4**

7. Harmonised standard:

 **EN998-1:2016**

8. Declared Performance

|  |  |  |
| --- | --- | --- |
| **Essential Characteristics** | **Performance** | **Harmonised Technical Standard** |
| Reaction to Fire | A1 | EN998 |
| Water Absorption | Wc1 | EN998 |
| Water Vapour Permeability | µ 15/35 | EN998 |
| Adhesion | >0.08 FP B | EN998 |
| Thermal Conductivity | 0.61 W(m.K) | EN998 |
| Durability | NPD | N/A |
| Dangerous Substances | Refer to MSDS | N/A |

9. The performance of the product identified above is in conformity with the set of declared performance/s. This declaration of performance is issued, in accordance with Regulation (EU) No 305/2011, under the sole responsibility of the manufacturer identified above.

Signed:

 

James Ayres Director

9/12/16